INFO ON THE TWO TEX FIN COOLERS

2 - Gas Cooler Type – Mfg. Tek-Fin, Inc., 2 bay, 1 fan per bay,
SN 1843-1A
Model 2-1736T12.5
Design: 1,300 PSIG 300º F/MDMT -20ºF
Connection Sizes: (2) 10”, 600 # Class, RF Inlets/ (2) 10”, 600 # Class, RF Outlets
Includes Fans and Fan Motors

